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YG119 Hunting Dog GPS Tracker

User Manual
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Hunting dog tracker is a rechargeable GPS tracker with long standby battery. Only need insert SIM card, it will upload GPS location based on movement or preset frequency automatically. 


Production Features
· Real time tracking via tracking APP
· Geo-fence/Low battery alarm
· Real time tracking/power saving/Deeply sleep mode.
· Find your pet via buzzer sound
· Electric shock training for dogs
· Magnet charging point
· Waterproof IP68

Specs.
	GSM Specification

	

4G LTE bands
	4G: 
LTE-FDD B1/B2/B3/B4/B5/B7/B8/B28/B66 
LTE-TDD B34/B38/B39/B40/B41 
2G:  GSM850/GSM900/1800/GSM1900

	GPRS
	Class 12, TCP/IP

	Memory
	32 + 32 Mb

	Phase error
	RMSPE<5,PPE<20

	Max output
	GSM850/GSM900:33±3dBm ,GSM1800/GSM1900:30±3dBm

	Max frequency error
	±0.1ppm

	Receive sensitivity
	Class II RBER2%(-102dBm)

	GPS Specification

	Chipset
	SIMCom LTE Cat 1 A7670SA + UC6228CI (GPS)

	Frequency
	GPS L1, 1575.42 MHz C/A code

	Channel
	66

	Location accuracy
	<5meters

	Tracking sensitivity
	-165dBm

	Acquisition sensitivity
	-148dBm

	TTFF (open sky)
	Avg. hot start ≤1 sec 

	
	Avg. cold start≤40 sec

	Others

	Antenna
	Built-in quad band GSM antenna, GPS ceramic antenna

	Charging voltage
	5VDC

	Working current
	2mA~78mA

	Electric shock current
	Instantaneous voltage 6800V

	Battery
	rechargeable 4500 lithium battery

	Standby time
	Everyday move 1 hour activities can standby 14 days

	Operating temperature
	-20℃~+60℃

	Unit Size
	78*40*44MM

	Waterproof
	IP68
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· Power on button




· Speaker/Microphone

· Electronic shock Point





· Charging Point




















Start Using
1. Insert a SIM card with 4g data activated.
2. Press the backside circle button 3 seconds to power on, and beep one time.
Press button 6 seconds to power off, and beep one time.
3. Put back back shell and tighten the screws for 100% waterproof
	Light
	Signal
	Normal
	Abnormal

	Green
	GSM
	Flashing
	Constant on

	Blue
	GPS
	Flashing
	Constant on

	Red
	Power 
	Constant on: charging
	Turn off: charged full

	Device will power off automatically during charging.




SMS Command List
	SMS Function
	SMS Command format
	SMS example

	· Please don’t type “+” “space”, password 123456
· Preset Center Number first before testing SMS or Phone Call alarm mode.
· Each SMS must reply“OK” represent command successfully.

	Mode 0
	mod123456+space+0
	Real time mode consume battery fast

	Mode 1
	mod123456+space+1
	Vibrate mode based on movement

	Mode 2
	mod123456+space+2
	Deeply sleep mode wakeup 3 minutes at every 2hrs

	Get location now
	DM123456
	Get current location update 1 time

	Find Pet via buzzer
	Find123456
	Buzzer sound 10seconds

	Set IP Port
	adminip+password+space+IP Address+space+port number
	[bookmark: OLE_LINK11][bookmark: OLE_LINK10]adminip123456 www.gps2828.com 7018

	Set APN
	apn123456+space+LocalApn+space+ApnName+space+ApnPassword
	apn123456 internet

	Set Time Interval
	ITV123456+space+time interval(s)
	If 60s , send SMS: ITV123456 60

	Set admin number
	Admin123456+space+PhoneNumber
	You can set max 5 numbers
Admin123456 13702581234 13702581235 13702581236

	Set low battery alarm
	lowbat123456+space+on
	lowbat123456 on

	Cancel low battery 
	lowbat123456+space+off
	lowbat123456 off

	Set SMS time zone
	Time+space+zone123456+space+X
	If+3,send sms time zone123456 3

	Check device status
	check123456
	check GPS GSM status

	Activate voice listen
	Monitor123456
	

	Cancel voice isten
	Tracker123456
	

	Set alarm mode
	KC123456+space+0
	Cancel alarm

	
	KC123456+space+1
	APP alarm (default)

	
	KC123456+space+2
	APP+SMS alarm

	Set factory mode
	begin123456
	It will erase all setting




[bookmark: _Toc6350]Real time Tracking Software

Web:    www.gps16888.com 
Android & IOS APP : toptrace
Default to use IMEI number login, password as 123456.
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