[bookmark: _GoBack]
Introduction to K6 product specifications
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Product Overview
   ● Product Name: K6-4G Bicycle Locator
   ● Application scenarios: bicycles, mountain bikes, and other cycling series
   ● Core functions: real-time positioning, historical track playback, electronic fence, wifi positioning, overspeed alarm, vibration alarm, low battery alarm, etc
   ● Product Highlights: High-precision positioning (5 meters), four-mode positioning (GPS + Beidou + LBS + WIFI), long battery life, strobe warning lights, and bracket installation
                  One-click car locator (with buzzer)


Technical Specifications
	project
	Function Name
	have
	none
	Functional Description

	Power Characteristics
	power supply method
	●
	
	battery-powered

	
	Operating voltage range
	●
	
	DC 3.45V - 4.35V

	
	operating current
	●
	
	3.7V/45mA (GPS upload for one minute)

	
	quiescent current
	●
	
	3.7V/4mA

	
	Built-in battery capacity
	●
	
	1500 mAh (3.8V polymer battery)

	Environmental characteristics
	Operating temperature range
	●
	
	-20℃ - 70℃

	
	Storage temperature range
	●
	
	-40℃ - 85℃

	
	Operating humidity range
	●
	
	5%-95%  

	Communication characteristics
	Communication module brand/chip model
	●
	 
	ASR1603S

	
	communication frequency band
	●
	
	GSM：900/1800MHZ
FDD-LTE:B1/3/5/8
TDD-LTE:B38/39/40/41

	
	SIM card
	●
	
	Nano SIM card

	
	communication antenna
	●
	
	Built-in FPC antenna

	GPS/BD positioning features
	Cold start time
	●
	
	On average, it takes 45 seconds

	
	Hot start time
	●
	
	On average, 1 second

	
	Sensitivity (tracking)
	●
	
	-165dbm

	
	positioning antenna
	●
	
	Built-in antenna FPC antenna

	Hardware function
	USB
	●
	
	Type-C, charging, activating battery

	
	LED
	●
	
	Strobe warning light

	
	buzzer
	●
	
	One-click car locating

	
	Gsensor
	●
	
	built-in

	
	GPS
	●
	
	Support global GPS and Beidou

	
	WiFi
	●
	
	WiFi positioning

	Outline specifications
	Host dimensions (length, width, height)
	●
	
	73mm × 60.5 mm × 29 mm

	
	Shell material
	●
	
	ABS plastic

	
	IP protection rating
	●
	
	IP65

	
	bicycle stand
	●
	
	ABS plastic + silicone gasket

	
	host weight
	●
	
	~85 grams





Software features
Real-time tracking: View real-time locations through the APP/Web terminal, with update frequencies adjustable in multiple modes (10 seconds to 3 minutes).
Electronic fence: Customize a security zone, and trigger an APP push alert when entering or exiting.
Historical track: Stores and replays movement paths within 180 days, supports exporting in KML/GPX formats.
Multi-account management: Supports family/team sharing of device permissions.
OTA upgrade: Remote wireless firmware upgrade, with continuous optimization of functions.
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