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Detailed specifications:
· Precise positioning, with an accuracy of 1.5 meters (the product supports Beidou III).
· GPS + Beidou + LBS + WIFI four-mode positioning.
· Practical functions: real-time positioning, latent positioning, vibration wake-up, and step counting positioning.
· Dismantling alarm, vibration alarm, displacement alarm, low battery alarm, fence exit alarm, overspeed alarm, etc.
· Small in size, easy to conceal, with strong magnetic attraction (optional).
Application fields:
Leased vehicles, credit vehicles, passenger vehicles, taxis, freight vehicles, cattle and sheep positioning management, valuables management, etc

Device parameters:
	project
	Function Name
	have
	none
	Functional Description

	Electrical Characteristics
	power supply method
	●
	
	battery-powered

	
	Operating voltage range
	●
	
	DC 3.45V - 4.35V

	
	operating current
	●
	
	22mA

	
	Standby current
	●
	
	About 30uA

	
	Online standby current
	●
	
	4.5mA

	
	Built-in battery capacity
	●
	
	10000mAh (3.8V polymer battery)

	Environmental characteristics
	Operating temperature range
	●
	
	-20℃ - 70℃

	
	Storage temperature range
	●
	
	-30℃ - 80℃

	
	Operating humidity range
	●
	
	5%-95%  

	Communication characteristics
	Communication module brand/chip model
	 ●
	 
	ML307A-DCLN-China Mobile IoT

	
	communication frequency band
	●
	
	TDD:B34/38/39/40/41,FDD:B1/3/5/8

	
	SIM card
	●
	
	Micro SIM card

	
	communication antenna
	●
	
	Built-in FPC antenna

	GPS/BD positioning features
	Positioning module brand/chip model
	●
	
	BGI GPS Beidou chip (supporting Beidou-3)

	
	Cold start time
	●
	
	Average 32 seconds

	
	Hot start time
	●
	
	Average: 1 second

	
	Sensitivity (tracking)
	●
	
	-162dBm

	
	positioning antenna
	●
	
	Built-in active ceramic GPS antenna

	external interface
	Loudspeaker output interface
	
	●
	

	
	I/O interface
	
	●
	

	
	ADC detection input interface
	
	●
	

	
	RS485 interface
	
	●
	

	
	RS232 interface
	
	●
	

	
	serial port
	●
	
	3.3V serial port channel 1

	
	CAN
	
	●
	

	
	K-line
	
	●
	

	Outline specification
	Host dimensions (length, width, height)
	●
	
	75mm × 57 mm × 31.5 mm

	
	Shell material
	●
	
	ABS plastic

	
	IP protection rating
	●
	
	IP65

	
	strong magnet
	●
	
	optional

	
	collar
	●
	
	optional

	
	host weight
	●
	
	About 199 grams
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Featured functions:
“Ultra-low power consumption design

- Multiple working modes to cater to different scenarios

- High-performance positioning chip(supporting Beidou 3 gen
-A-Guss rapid positioning technology
~4G full network compatibility

- Electronic fence

- Historical trajectory

- Disarm alarm,low battery alarm,vibration alarm




