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	Elderly care tracker
	Supports TDD/FDD/GSM mobile network access services, GPS positioning, Beidou positioning, and WIFI positioning
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	Overall dimensions
	68*38*20 mm

	
	button
	Option 1: Power button (compatible with SOS function)
Option 2: Customized buttons for BTB connector: including power button, LED indicator, on/off switch, SOS, and others
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	FDD/TDD
	The upstream rate is 5Mbps, and the downstream rate is 10Mbps

	
	GSM
	The upstream rate is 48kbps, and the downstream rate is 54kbps

	

	B1,3,5,8
	

	
	B38,39,40,41
	

	
	900/1800MhZ
	

	

	Beidou
	1561.098MHz

	
	GPS
	1575.42MHz

	

	Acquisition
	-148dBm(cold)/-163dBm(hot)

	
	Tracking (tracking)
	-165dBM

	
	power consumption
	Acq:37mW,Tracking:27mW

	
	support
	Obtain MAC address, save power
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	support
	Optional, Bluetooth anti-lost feature

	


	Working Voltage
	3.5-4.2V DC

	
	voltage fluctuation
	3.3-4.5V DC

	
	operating current
	Sleep 0.3mA (maintain clock)
Standby 3.3mA (3-minute heartbeat), positioning 60mA (LTE+GPS)

	
	Built-in battery
	1500mAh high-voltage high-capacity polymer lithium battery

	

	Operating Temperature
	-20℃~+70℃

	
	Ultimate operating temperature
	-30℃~+75℃

	
	Storage temperature
	-40℃~+85℃

	
	relative humidity
	5%~95%
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	Gsensor
	built-in

	
	GPS
	Support global GPS and Beidou

	
	LED indicator light
	GPS (blue), GSM (green), Power (red)

	
	SIM interface
	Nano, push-push side insertion, compatible with 2*2 eSIM

	
	USB
	Option 1: Type-C, charging + downloading, testing, activating battery
Option 2: Magnetic attraction function, utilizing the 10-pin connector of the motherboard

	
	Simulated voice
	Built-in single microphone (interrupt detection + recording), with options for surface mount or wire bond depending on appearance

	
	horn
	8Ω, 1.2W or 4Ω, 2.4W

	
	watchdog
	Support, chip comes with it

	
	
antenna
	GPS: FPC or LDS (with spring clips on the mainboard)
LTE: FPC or LDS (mainboard with spring clip) WIFI: the mainboard comes with a ceramic patch antenna

	

[image: ]
	Smart wake-up/sleep
	Support, timing or Gsensor

	
	positioning
	Support, scheduled positioning, intelligent positioning, and super power-saving positioning

	
	WIFI positioning
	support

	
	Bluetooth anti-lost
	support

	
	Anti-theft recording
	support

	
	FOTA
	support
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