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Product Name
	
NY high-capacity positioning
	
Supports TDD/FDD/GSM mobile network access services, GPS positioning, Beidou positioning, and WIFI positioning

	structural characteristics
	Overall dimensions
	122*84*48.5mm

	
	Unit Weight
	400g/551g

	data services
	FDD/TDD
	Upstream rate of 5Mbps, downstream rate of 10Mbps

	
	GSM
	The upstream rate is 48kbps, and the downstream rate is 54kbps

	   Communication network frequency band
	Full Netcom
	China Mobile, China Unicom, China Telecom

	
	FDD frequency band
	B1,3,5,8

	
	TDD frequency band
	B38,39,40,41

	
	GSM frequency band
	900/1800MhZ

	GPS frequency band
	Beidou
	1561.098MHz

	
	GPS
	1575.42MHz

	
GPS sensitivity
	Acquisition
	-148dBm(cold)/-163dBm(hot)

	
	Tracking (tracking)
	-165dBM

	
	power consumption
	Acq:37mW,Tracking:27mW

	WIFI function
	support
	Obtain MAC address, save power

	

Power Characteristics
	Working Voltage
	3.5-4.2V DC

	
	voltage fluctuation
	3.3-4.5V DC

	
	
operating current
	Sleep 0.3mA (maintaining clock) Standby 3.3mA (3-minute heartbeat)
Positioning 60mA (LTE+GPS)

	
	Built-in battery
	10000mAh/20000mAh

	
Environmental characteristics
	Operating Temperature
	-20℃～+70℃

	
	Ultimate operating temperature
	-30℃～+75℃

	
	Storage temperature
	-40℃～+85℃

	
	relative humidity
	5%～95%

	





Main hardware functions
	Gsensor
	built-in

	
	GPS
	Support global GPS and Beidou

	
	solar energy
	

	
	LED indicator light
	GPS (blue), GSM (green), Power (red)

	
	SIM interface
	Nano, push-push side insertion, compatible with 5*6 ESIM

	
	USB
	Type-C, charging + downloading, testing, activating battery

	
	Simulated voice
	Built-in dual microphones (interruption detection + recording)

	
	watchdog
	Support, built-in chip

	
	
antenna
	GPS: Passive dual-mode ceramic 18*18; LTE: FPC (with spring clips on the mainboard)
WIFI: FPC (mainboard with spring clip)

	

Main software functions
	Smart wake-up/sleep
	Support, timing or Gsensor

	
	positioning
	Support, scheduled positioning, intelligent positioning, super power-saving positioning

	
	WIFI positioning
	support

	
	Anti-theft recording
	support

	
	FOTA
	support



image1.png
1x 50—

Mm. m i





